pop pop pop 1 2 3 3

4

5

6 CCD0, full chip 2x2 (w/ linear fit)